Risk assessment
✓  A competent person checks this against the site and signs it before work starts.
	Site or project
	
	Work assessed
	

	Client
	
	Principal contractor
	

	Assessed by
	
	Checked by (competent person)
	

	Date
	
	Next review
	


1. Who might be harmed
Tick everyone the work could affect, and note anyone at particular risk.
	☐  Your workers
	☐  Young workers

	☐  Other contractors on site
	☐  New or expectant mothers

	☐  Visitors and delivery drivers
	☐  Workers with a disability

	☐  Members of the public
	☐  Workers new to the site or the country

	☐  People using the building
	


Notes on anyone at particular risk:
	


2. Risk rating
Score each hazard before and after the controls: how likely it is, times how bad it could be.
	Severity
	1 Unlikely
	2 Possible
	3 Likely

	1 Minor injury
	1
	2
	3

	2 Injury or ill health with time off work
	2
	4
	6

	3 Major injury, lasting ill health or death
	3
	6
	9



	Risk
	Score
	What to do

	Low
	1 to 2
	Keep the controls in place.

	Medium
	3 to 4
	Reduce it further where you reasonably can.

	High
	6 to 9
	Don't start until it's lower.


3. Choosing controls
Start at the top and work down. Protecting everyone comes before protecting one person.
	1
	Remove the hazard
	Do the work another way, or somewhere safer, such as on the ground

	2
	Replace it
	With a less hazardous material, tool or method

	3
	Keep people away from it
	Barriers, guard rails, edge protection, on-tool extraction

	4
	Organise the work
	Sequence, time limits, permits, supervision and training

	5
	Personal protective equipment
	The last line, once everything above is in place
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4. Hazards and controls
One row per hazard. Rate the risk before and after the controls. Use the risk rating in part 2.
	Hazard
	Who might be harmed and how
	Controls in place
	Risk before
	Further controls needed
	Risk after
	Action by
	By when

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	



5. Briefing record
Everyone doing the work is told the hazards and controls before starting, and signs here.
	Name
	Company
	Signature
	Date

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	


6. Review record
Review it when the work, the team, the equipment or the site changes, and after any accident or near miss.
	Date
	What changed
	Changes made to this assessment
	Reviewed by

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	


7. Sign-off
A competent person checks this against the site and signs it before work starts.
	
	Name
	Position
	Signature
	Date

	Assessed by
	
	
	
	

	Checked by (competent person)
	
	
	
	

	Accepted by principal contractor (if required)
	
	
	
	






